/* Architecture and core descriptions for the C-SKY back end.
   Copyright (C) 2018-2020 Free Software Foundation, Inc.
   Contributed by C-SKY Microsystems and Mentor Graphics.

   This file is part of GCC.

   GCC is free software; you can redistribute it and/or modify it
   under the terms of the GNU General Public License as published
   by the Free Software Foundation; either version 3, or (at your
   option) any later version.

   GCC is distributed in the hope that it will be useful, but WITHOUT
   ANY WARRANTY; without even the implied warranty of MERCHANTABILITY
   or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public
   License for more details.

   You should have received a copy of the GNU General Public License
   along with GCC; see the file COPYING3.  If not see
   <http://www.gnu.org/licenses/>.  */

/* Before using #include to read this file, define a macro:

      CSKY_ARCH(NAME, CORE, ARCH, ISA)

   The NAME is the name of the architecture, represented as a string
   constant.  The CORE is the identifier for a core representative of
   this architecture.  ARCH is the architecture revision.  ISA is the
   detailed architectural capabilities of the core.  */

#ifdef CSKY_ARCH
CSKY_ARCH ("ck801",  ck801,  CK801,
	   CSKY_ISA_FEAT (CSKY_ISA_CK801))
CSKY_ARCH ("ck802",  ck802,  CK802,
	   CSKY_ISA_FEAT (CSKY_ISA_CK802))
CSKY_ARCH ("ck803",  ck803,  CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_CK803))
CSKY_ARCH ("ck807",  ck807,  CK807,
	   CSKY_ISA_FEAT (CSKY_ISA_CK807) CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_ARCH ("ck810",  ck810,  CK810,
	   CSKY_ISA_FEAT (CSKY_ISA_CK810) CSKY_ISA_FEAT (CSKY_ISA_DSP))
#endif


/* Before using #include to read this file, define a macro:

      CSKY_CORE(CORE_NAME, INTERNAL_IDENT, TUNE_IDENT, ARCH, ISA)

      The isa features of core will inherit the ARCH.

   The CORE_NAME is the name of the core, represented as a string constant.
   The INTERNAL_IDENT is the name of the core represented as an identifier.
   This must be unique for each entry in this table.
   The TUNE_IDENT is the name of the core for which scheduling decisions
   should be made, represented as an identifier.
   The ARCH is the architecture revision implemented by the chip.
   The ISA is the detailed architectural capabilities of the core.  */

#ifdef CSKY_CORE
/* ck801 Architecture Processors */
CSKY_CORE ("ck801",    ck801,	 ck801,	   CK801,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck801t",   ck801t,	 ck801t,   CK801,
	   CSKY_ISA_FEAT_NONE)

/* ck802 Architecture Processors */
CSKY_CORE ("ck802",    ck802,	 ck802,	   CK802,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck802t",   ck802t,	 ck802t,   CK802,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck802j",   ck802j,	 ck802j,   CK802,
	   CSKY_ISA_FEAT (isa_bit_java))

/* ck803 Architecture Processors */
CSKY_CORE ("ck803",    ck803,	 ck803,	   CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803h",   ck803h,	 ck803h,   CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803t",   ck803t,	 ck803t,   CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803ht",  ck803ht,	 ck803ht,  CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803f",   ck803f,	 ck803f,   CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803fh",  ck803fh,	 ck803fh,  CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803e",   ck803e,	 ck803e,   CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803eh",  ck803eh,	 ck803eh,  CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803et",  ck803et,	 ck803et,  CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803eht", ck803eht, ck803eht, CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803ef",  ck803ef,	 ck803ef,  CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803efh", ck803efh, ck803efh, CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803ft",  ck803ft,	 ck803ft,  CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803eft", ck803eft, ck803eft, CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803efht", ck803efht, ck803efht, CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803r1",	 ck803r1,    ck803r1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803hr1",	 ck803hr1,   ck803hr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803tr1",	 ck803tr1,   ck803tr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803htr1",	 ck803htr1,  ck803htr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803fr1",	 ck803fr1,   ck803fr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803fhr1",	 ck803fhr1,  ck803fhr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803er1",	 ck803er1,   ck803er1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803ehr1",	 ck803ehr1,  ck803ehr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803etr1",	 ck803etr1,  ck803etr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803ehtr1", ck803ehtr1, ck803ehtr1, CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803efr1",	 ck803efr1,  ck803efr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803efhr1", ck803efhr1, ck803efhr1, CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803ftr1",	 ck803ftr1,  ck803ftr1,	 CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803eftr1", ck803eftr1, ck803eftr1, CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))
CSKY_CORE ("ck803efhtr1", ck803efhtr1, ck803efhtr1, CK803,
	   CSKY_ISA_FEAT (isa_bit_3E3r1))

/* ck803s Architecture Processors */
CSKY_CORE ("ck803s",   ck803s,	 ck803s,   CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803st",  ck803st,	 ck803st,  CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803se",  ck803se,	 ck803se,  CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803sf",  ck803sf,	 ck803sf,  CK803,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck803sef", ck803sef, ck803sef, CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))
CSKY_CORE ("ck803seft", ck803seft, ck803seft, CK803,
	   CSKY_ISA_FEAT (CSKY_ISA_DSP))

/* ck807 Architecture Processors */
CSKY_CORE ("ck807e",   ck807e,	 ck807e,   CK807,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck807ef",  ck807ef,	 ck807ef,  CK807,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck807",    ck807,	 ck807,	   CK807,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck807f",   ck807f,	 ck807f,   CK807,
	   CSKY_ISA_FEAT_NONE)

/* ck810 Architecture Processors */
CSKY_CORE ("ck810e",   ck810e,	 ck810e,   CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810et",  ck810et,	 ck810et,  CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810ef",  ck810ef,	 ck810ef,  CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810eft", ck810eft, ck810eft, CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810",    ck810,	 ck810,	   CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810v",   ck810v,	 ck810v,   CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810f",   ck810f,	 ck810f,   CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810t",   ck810t,	 ck810t,   CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810fv",  ck810fv,	 ck810fv,  CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810tv",  ck810tv,	 ck810tv,  CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810ft",  ck810ff,	 ck810ft,  CK810,
	   CSKY_ISA_FEAT_NONE)
CSKY_CORE ("ck810ftv", ck810ftv, ck810ftv, CK810,
	   CSKY_ISA_FEAT_NONE)
#endif


/* Before using #include to read this file, define a macro:

      CSKY_FPU(NAME, CNAME, ISA)

   NAME is the publicly visible option name.
   CNAME is a C-compatible variable name substring.
   ISA is the list of feature bits that this FPU provides.  */

#ifdef CSKY_FPU
CSKY_FPU ("fpv2_sf",   fpv2_sf,	  CSKY_ISA_FEAT (CSKY_ISA_FPv2_SF))
CSKY_FPU ("fpv2",      fpv2,	  CSKY_ISA_FEAT (CSKY_ISA_FPv2))
CSKY_FPU ("fpv2_divd", fpv2_divd, CSKY_ISA_FEAT (CSKY_ISA_FPv2_DIVD))
#endif
